**Hear Protector with BluetoothTM**

**USER INSTRUCTION MANUAL**

**Thank you for purchasing a Rifleman Bluetooth Hearing Protector. This hearing protector is designed to reduce exposure to harmful noise. To get the best performance please read this user manual carefully before using the unit. Save the manual for future reference.**

**Components**

1. **Battery Compartment Cover 2.Auxiliary Input**
2. **Microphone 4 Multi Function Button (MFB).**
3. **Vol Up / Skip Fwd 6. Vol Down/Skip Back**
4. **Indicator light 8. Ear Cushions**
5. **Sliders**



**OPERATION:**

A) *Adjust for Fit* - Headband may be adjusted to ensure cups fit correctly around the ears by sliding headband apart. With the slider arms retracted place the headband directly in the middle of the head. Slowly adjust one slider arm at a time as needed to ensure each cup is fully covering your ear. The two slider arms should extend an equal distance from the headband to ensure best fit. Be sure the headband is resting snuggly against the top of your head. There should be no gaps between the ear seal and your head. For best fit ensure your hair is not under the ear seal. To test for a good seal, run your index finger around the area between the ear seal and your skull and ensure there are no gaps.

B). *Batteries* - Slide battery compartment cover to reveal the battery compartment. Requires three 'AAA' size batteries. Alkaline batteries provide the best service. Remove the old batteries, place new batteries with the negative to negative and positive to positive side. The correct polarity is marked on the holders. Once batteries are installed, carefully replace the battery cover.

C). *On / Off* To turn on the unit press and hold the MFB for 2 seconds or until you hear “power on, Pairing” through the speakers. The indicator light will flash blue to indicate the power is on

To power off press and hold the MFB for 3 seconds or until you hear “power off”.

D) BluetoothTM Pairing – Press and hold the MFB until the indicator light flashes red and blue or until you hear “pairing”. The headset must be within 3 meters of the device you are pairing with. Search and select the new device. You will hear “paired” when pairing is successful. You are now ready to play music or accept phone calls. After powering off and powering back on again the headset will automatically reconnect with your device if within range.

E) *Audio Control* – Press and hold the Vol Up (5) + or the Vol Down (6) – for 1 second to adjust the volume.

Play and Pause music. Momentarily press the MFB to pause playback, press again to resume playback.

Forward / Backward song selection. Momentarily press either Skip (5) + or Skip (6) – button to advance forward or backward.

F)*. Phone Call Functions* – Answering Calls – Momentarily press the MFB once to accept a call. Press and hold for 2 seconds to decline a call. Ending calls – Momentarily press the MFB once to end a call. Last Number Redial – Press the MFB twice to redial the last number dialed.

G).*Auxiliary Functio*n – Connect external audio through the auxiliary input (2) using a 3.5mm stereo cord (not included). Once an external audio device is connected the Bluetooth TM function automatically powers off. If an external device is connected the volume and playback function is controlled by your device.

(H) Battery Life – When the battery life is low the indicator light (7) will flash red accompanied by periodic beeps. You can expect 50 – 60 hours of playback from a fresh set of alkaline batteries, depending upon use.

**IMPORTANT!**

1). Rifleman hearing protectors are extremely durable however it is not advisable to expose them to extreme heat or cold or direct moisture as this can damage the electronics.

2). Check to ensure batteries are in good condition.

**TROUBLE SHOOTING:**

1. We recommend removing the batteries for replacement by placing an object (knife, screw driver, etc) under the lip at the end of the battery and carefully applying enough pressure to ease the battery up and out of the compartment.
2. This is an electrical device and all effort should be made to protect against exposure to excessive moisture from rain, snow, etc. Should the unit be exposed to moisture it will be necessary to allow the unit to dry overnight, naturally. If this is done, the unit should work normally once fully dried. CAUTION: NEVER DRY WITH AN ELECTRONIC HAIR DRYER OR OTHER ARTIFICIAL MEANS. THIS COULD RESULT IN DAMAGE TO THE UNIT!
3. After an extended period of use the Sealing Rings should be replaced.
4. It is recommended that your hearing protector be placed in a protective bag or hard case for storage and travel to protect its appearance.

**NOISE REDUCTION RATING**

The Environmental Protection Agency has selected the NRR as the measure of a hearing protector’s attenuation capability. Rifleman makes no warranties as to the suitability of NRR as a measure of actual protection from noise since protection depends on the sound level, duration and fit. .NRR may not be a good indicator of protection against impulse noise such as gunfire. We highly recommend users wear ear plugs under the ear muffs for added protection in high noise environments. **IMPROPER FIT WILL REDUCE EFFECTIVENESS!**



**ANSI S 3:19-1974**

Example

1. The environmental noise level as measured at the ear is 92 decibels (dBA)
2. The NRR is 25 dBA
3. The level of noise entering the ear is approximately 67 dBA

Caution For noise environments dominated by frequencies below 500 hz the C-weighted environmental noise level should be used.

**Audio Input Level**

If your unit is connected to an external device you are responsible to set the audio input to a safe level.

**Warranty**

This unit is warrantied to be free of defects in material and workmanship for a period of ninety days from the date of original purchase. Rifleman will at its sole discretion repair or replace without charge, except for transportation costs, parts that fall under normal use and service. This warranty does not cover damage caused by mis use, abuse or unauthorized modifications. Proof of purchase is required to verify eligibility. Contact Customer Service to get an RMA before returning the product for evaluation.

Altus Brands, a Grawn MI company. 1.800.891.3660 customerservice@altusbrands.com